2010년 제9차 국내 미생산 확인 제품(2010.12.27)

신청자	생산자/국가	제품명	형식명	정격	적용표준
㈜씨이씨코리아	ARTECHE /스페인	Indicator & Relay	VU3	48-110-125Vdc	IEC 60255/60068, EN 61810-7
			RPT	48-110-125Vdc	IEC 60255/60068
	P&B ENG. /영국	Protection Relay	Feeder vision Series (Drawout, Non-drawout)	25/27/36/50/51/51n/59/74/81/48A/TCS	IEC 60255
			Motor vision Series (Drawout, Non-drawout)	9/19/34/79/14/48/27/32/37/38/49/46/47/50/51/50n/51n/55/59/66/74/81/86/RTD, TCS, MPR	“
			Micro motor	14/48/27/32/38/49T/46/47/50/51/50n/55/59/66/74/81/86/RTD	“
			MPR3E5	26/37/46/46SP/49/50/51/50n/51n/74/66 (non voltage element)	IEC 60255, EN 50082, ENV 50140
			MPR2000/ 3000	23/27/30/37/38/46/48/49/50/51/50n/51n/59/RTD	IEC 60255, EN 55022/55011, ENV 50204
			MR-CS	25(Diffrential type)	“
			MRDT	87T(TR differential type)	IEC 60255/61000 /60068
			MIRD-T	87T(TR differential type)	“
			MRDG	87G(Gen differential type)	“
			MRRP	32(32PQ differential type)	IEC 60255/61000 /60068
			MRFT	81UO(differential type)	“
	WOODWARD KEMPEN/독일	Protection Relay	MRA4	46/49/81uo/74/74TC (Feeder Multi type)	“
			MRD1-T	87T(TR differential type)	“
			MRD1-G	87G(Gen differential type)	“
			WI Series	50/51/50n/51n (Self power type)	“
			SPM-D10	25(Synchronizing unit for power Gen&mani)	“
㈜씨이씨코리아	WOODWARD KEMPEN/독일	Protection Relay	CSP-F	50/51/67/50n/51n/67n/46/49/27/59/59n/ 81/32FR/79/86/74TC/ 50BF (Feeder Multi type)	“
			CSP-T	50/51/67/50n/51n/67n/49/27/59/59n/87T/79/86/74TC/50BF	“
			CSP-L	50/51/67/50n/51n/67n/27/59/59n/87L/79/86/74TC/50BF	“
			CSP-B	87B/50BF	“
			MRP Series	32P, 32Q, 37	“
			MRF3	81(81UO)	“
			XRN2	27/59/81UO/78	“
			MRS1	46(for Generator)	“
			MRR1	64n, 40/76 (for Generator)	“
			MRQ1	40(for Generator)	“
			IRI1	64REF	“
			MRN3	27/59/50/51/50n/51n/78/81/47	IEC 60255, EN 50263
			MRG3	50/51/50n/51n (for Generator)	IEC 60255/61000 /60068
			MRDT4	46/49/64REF/74TC/86 TR(Generator Multi type)	IEC 61850, IRIG port

주) 정격의 숫자는 ANSI 계전요소 번호임