『인도 전력표준 수요조사』

귀사의 무궁한 발전을 기원합니다.

현재 한국의 전력산업은 고유가와 국내시장 포화 등 대내외적으로 어려운 상황에 직면하고 있습니다. 이에 보다 적극적인 해외시장 진출 등이 요구되고 있는 시점이며, 해외시장 진출시 그 나라의 기술표준, 제품의 개발, 시험․인증 등 전력산업과 관련한 전문적인 정보는 사업추진에 있어 매우 중요한 요소입니다

우리협회에서는 국내 전력기자재 제조업체의 인도 등 아시아 신흥공업국 전력시장 진출을 활성화하고, 진출시 손실비용을 최소화 하고자 “아시아 신흥공업국 전력시장 수출촉진을 위한 시장조사 및 기술표준 검토서 개발”연구를 수행하고 있습니다. 이는 국내 전력기자재 제조업체에 해외 시장진출시 필요한 전문자료를 제공하여 기술경쟁력 향상 및 수출촉진에 기여할 것입니다.

따라서 전력기자재 제조업체를 대상으로 필요한 분야의 인도 전력기술표준에 대한 수요조사를 실시하여 실질적이고 유용한 결과물을 도출하고자 하오니 붙임의 “인도 전력표준 수요조사”서를 작성하시어‘11. 09. 09일까지 회신하여 주시기 바랍니다. 본 수요조사에 성실히 응답하여 주신 기업에는 설명회 초청 및 결과물 제공시 우선적으로 배포하여 드리겠습니다.

감사합니다.

[문의 및 회신]

대한전기협회

주소 : 100-230 서울 중구 수표동 11-4(전기회관)

기술기준처 신대성 과장

TEL : 02-3393-7662, FAX : 02-3393-7689

E-mail : shinds@electricity.or.kr

※ 결과물 배포를 위해 아래사항을 작성하여 주시기 바랍니다.

업 체 명	:
응답자 성명	:		부서명	:		직 위	:
전화번호	:		e-mail	:
주 소	:

인도 전력표준 수요조사

Ⅰ. 인도 전력시장 정보 제공 우선순위

1. 인도 전력표준과 관련하여 귀사가 가장 필요로 하는 정보는 무엇입니까?

(복수응답 가능)

① 인도 국가표준, 인도 전력표준 번역본

② 인도 국가표준, 인도 전력표준, 국내 한전표준 등과 IEC표준 비교표

③ 인도 전력시장에 대한 정보

④ 제품·구매인증제도

2. 상기 1번의 질문에 예시된 기술표준 및 정보자료 이외에 귀사 제품의 인도 수출 또는 인도 시장 진출과 관련하여 추가로 필요로 하는 정보를 기술하여 주십시오.

① 시장 규모(향후 몇 년간)

② 가격 경쟁력

③ 시장 진입가능성 여부

④ 시장 참여 가능 품목 등

⑤ ___________________________________________________________________

Ⅱ. 개발 수요조사

3. 전력기자재 중 인도에 수출을 희망하고 있거나 유망하여 인도의 기술표준 검토가 필요하다고 생각되는 품목을 선택하여 주십시오.

제품군	품목	선택	대응 국제표준
차단기 및 개폐장치	고압진공 차단기
	큐비클형 가스절연 개폐장치
	옥내 교류 폐쇄배전반
	교류 고압 자동재폐로 차단기
	교류 고압부하개폐기
	단로기 및 접지개폐기
	고장구간 자동개폐기
	부하개폐기-퓨즈 조합장치
	교류 고압퓨즈
	조립식 변전소
	기타 1. _____________________________
	기타 2. _____________________________
	기타 3. _____________________________
변압기류	전력용 유입식 변압기
	전력용 건식 변압기
	전압변성기
	전류변성기
	기타 1. _____________________________
	기타 2. _____________________________
	기타 3. _____________________________

제품군	품목	선택	대응 국제표준
계전기 및 전력 자동화장치	계전기 및 계전장치
	원격단말장치
	배전자동화시스템
	기타 1. _____________________________
	기타 2. _____________________________
	기타 3. _____________________________
케이블 및 피뢰기	폴리머 피뢰기
	220 kV XLPE 케이블 및 접속장치
	광섬유 복합가공지선
	기타 1. _____________________________
	기타 2. _____________________________
	기타 3. _____________________________
애자 및 금구류	폴리머 애자
	고압부싱
	가공배전선로 금구류
	스페이서 댐퍼
	기타 1. _____________________________
	기타 2. _____________________________
	기타 3. _____________________________
기타 ___________	기타 1. _____________________________
	기타 2. _____________________________
	기타 3. _____________________________

4. 전력기자재중 인도에 수출을 희망하고 있거나 유망하여 인도의 기술표준 번역이 필요하다고 생각되는 품목을 선택하여 주십시오.

가. 차단기 및 개폐장치

표준번호	제목	검토	번역
IS 10118(1982)	Code of Practice for Selection, Installation and Maintenance of Switchgear and Controlgear - Part I : General
IS 10601(1983)	Dimensions of terminals of high voltage switchgear and controlgear
IS 11353(1985)	Guide for Uniform System of Marking and Identification of Conductors and Apparatus Terminals [IEC Pub 60445:1973]
IS 12021(1987)	Specification for Control Transformers for Switchgear and Controlgear for Voltages not Exceeding 1000 V ac
IS 12729(2004)	Common High-Voltage Switchgear and Controlgear Standards [IEC 60694 : 2002]
IS 13118(1991)	High-Voltage Alternating-Current Circuit-Breakers [IEC 60056: 1987]
IS 13516(1993)	Methods of Synthetic Testing of High Voltage Alternating Current Circuit-breakers [IEC 60427 :1989]
IS 13947-1(1993)	Low-voltage Switchgear and Controlgear - Part 1 : General Rules
IS 13947-2(1993)	Low-voltage Switchgear and Controlgear - Part 2 : Circuit Breakers
IS 14657(1998)	Gas insulated metal enclosed switchgear for rated voltages 72.5 kV and above - requirements for switching of bus-charging currents by disconnectors [IEC 1259(1994)]
IS 14658(1998)	High Voltage Alternating Current Circuit Breakers - Guide for Short-circuit and Switching Test Procedures for Metal-enclosed and Dead Tank Circuit Breakers[IEC 1633(1995)]
IS 14659(1999)	A. C. Insulation-Enclosed Switchgear and Controlgear for Rated Voltages Above 1 kV and up to and Including 38 kV [IEC 60466 : 1987]
IS 14666(1999)	High-voltage Alternating Current Switch-fuse Combinations[IEC 60420(1990)]
IS 14674(1999)	High Voltage Alternating Current Circuit-breakers -guide for Seismic Qualification of High Voltage Alternating Current Circuit-breakers[IEC 1166(1993)]
IS 14674(1999)	High Voltage Alternating Current Circuit-breakers -guide for Seismic Qualification of High Voltage Alternating Current Circuit-breakers [IEC 1166 : 1993]
IS 14786(1999)	High-Voltage/Low-Voltage Prefabricated Substations [IEC 61330(1995)]
IS 2147(1962)	Degrees of protection provided by enclosures for low voltage switchgear and controlgear
IS 2544(1973)	Porcelain post insulators for systems with nominal voltage greater than 1000 Volts [IEC 60168(1964)]
IS 2633(1986)	Methods for testing uniformity of coating of zinc coated articles
IS 3427(1997)	A.C. Metal Enclosed Switchgear and Controlgear for Rated Voltages Above 1 kV and Up to and Including 52 kV [IEC 286(1990)]
IS 5561(1970)	Electric Power Connectors
IS 7567(1993)	Automatic circuit reclosers
IS 8623-1(1993)	Low-Voltage Switchgear and Controlgear Assemblies - Part 1 : Requirements for Type-Tested and Partially Type-Tested Assemblies [IEC 439-1: 1985]
IS 8623-2(1993)	Low-voltage Switchgear and Controlgear Assemblies - Part 2 : Particular Requirements for Busbar Trunking Systems [IEC 439-2: 1987]
IS 9135(1979)	Guide for testing of circuit breakers with respect to out-of-phase switching
IS 9920-1(2002)	High Voltage Switches - Part 1 : Switches for Rated Voltages Above 1 kV and Less Than 52 kV[ISO 4099(1984)]
IS 9920-1(2002)	High Voltage Switches - Part 1 : Switches for Rated Voltages Above 1 kV and Less Than 52 kV [IEC 60265-1]
IS 9920-2(1985)	High Voltages Switches : Part II High Voltage Switches for rated Voltages of 52 kV and above Rating [IEC 60265-2]
IS 9920-2(2001)	High Voltages Switches : Part II High Voltage Switches for rated Voltages of 52 kV and above Rating[ISO 14673-1(2004)]
IS 9920-3(1985)	Specification for Alternating Current Switches for Voltages Above 1000 V - Part III : Design and Construction
IS 9920-4(1985)	Specification for Alternating Current Switches for Voltages Above 1000 V - Part 4 : Type Tests and Routine Tests
IS 9921-1(1981)	Specification for Alternating Current Disconnectors (Isolators) and Earthing Switches for Voltages Above 1000 V - Part I : General and Definitions [IEC 60129(1975)]
IS 9921-2(1982)	Alternating current disconnectors (isolators) and earthing switches for voltages above 1000 V: Part 2 Rating [IEC 60129(1975)]
IS 9921-3(1982)	Specification for Alternating Current Disconnectors (Isolators) and Earthing Switches for Voltages Above 1000 V - Part III : Design and Constructions [IEC 60129(1975)]
IS 9921-4(1985)	Specification for Alternating Current Disconnectors (isolators) and Earthing Switches for Voltages Above 1000 V - Part 4 : Type Tests and Routine Tests [IEC 60129(1975)]
IS 9921-5(1985)	Specification for Alternating Current Disconnectors (Isolators) and Earthing Switches for Voltages Above 1000 V - Part 5 : Information to be Given with Tenders, Enquiries and Orders [IEC 60129(1975)]
기타 1.
기타 2.
기타 3.

나. 변압기

표준번호	제목	검토	번역
IS 1271(1985)	Thermal Evaluation and classification of Electrical Insulation. [IEC 60085(1984)]
IS 335(1993)	New insulating oils [BS 148, D-1473, D-1533- 1934 IEC Pub 296-1969]
IS 3639(1966)	Fittings & Accessories for Distribution Transformers
IS 6600(1972)	Guide for loading of Oil Immersed Transformer [IEC 60076]
IS 10028-2(1981)	Code of practice for selection, installation and maintenance of transformers; Part 2 Installation
IS 11171(1985)	Specification for Dry-Type Power Transformers[IEC 60727(1982)]
IS 11333(1985)	Specification for Flameproof Dry Type Transformers For Use in Mines
IS 1180-1(1989)	Outdoor type three-phase distribution transformers up to and including 100 kVA 11 kV; Part 1 Non-sealed type
IS 1180-2(1989)	Outdoor type three-phase distribution transformers up to and including 100 kVA 11 kV; Part 2 Sealed type
IS 12444	Specification for Copper wire rod [ASTM B 49]
IS 13964(1994)	Methods of measurement of transformer and reactor sound levels [IEC 551(1976)]
IS 1576	Specification for Insulating Press Board [IEC 60641]
IS 1866	Code of practice for maintenance & supervision of Mineral insulating oil in equipment [IEC 60296:1982]
IS 2026-1(1977)	Power transformers: Part 1 General [IEC 60076 (1977)]
IS 2026-10(2009)	Power Transformers : Part 10 Determination of sound levents [IEC 60076-10(2001)]
IS 2026-2(2010)	Power transformers Part 2 Temperature-rise
IS 2026-3(1981)	Power transformers: Part 3 Insulation level and dielectric tests [IEC 60076(1977)]
IS 2026-4(1977)	Power transformers: Part 4 Terminal marking, tappings and connectioins [IEC 60076(1977)]
IS 2026-5(1994)	Power Transformer: Part 5 Transformer/Reactor bushings minimum external clearance in air- specification [IEC 60076-3-1(1987)]
IS 2026-7(2009)	Power Transformers Part 7 Loading Guide for Oil-Immersed Power Transformers [IEC 60076-7]
IS 2026-8(2009)	Power Transformer: Part 8 Applications guide Transformer/Reactor bushings minimum external clearance in air-specification [IDR IEC 60076-8(1997)]
IS 2705-1(1992)	Current transformers: Part 1 General requirements [IEC 60185:1966]
IS 2705-2(1992)	Current transformers: Part 2 Measuring current transformers [IEC 60185:1966]
IS 2705-3(1992)	Current transformers: Part 3 Protective current transformers [IEC 60185:1966]
IS 2705-4(1992)	Current transformers: Part 4 Protective current transformers for special purpose applications[IEC 60185:1966]
IS 3156-1(1992)	Vltage transformers: Part 1 General requirements [IEC 60186:1987]
IS 3156-2(1992)	Voltage transformers: Part 2 Measuring voltage transformers [IEC 60186:1987]
IS 3156-3(1992)	Voltage transformers: Part 3 Protective voltage transformers [IEC 60186:1987]
IS 3156-4(1992)	Voltage transformers: Part 4 Capacitor voltage transformers [IEC 60186:1987]
IS 3401(1992)	Silica gel
IS 4257-1(1981)	Dimensions for Clamping Arrangements for Porcelain Transformer Bushings - Part I : For 12 kV to 36 kV Bushings
IS 4257-2(1986)	Dimensions for clamping arrangements for porcelain transformer bushings: Part 2 For 72.5 kV and 123 kV bushings
IS 5(1961)	Specification for colors for ready mixed paints
IS 5484	Specification for Al Wire rods [ASTM B 233]
IS 5553-1(1989)	Reactors - Specification - Part 1 : General [IEC 60289(1988)
IS 5553-2(1990)	Reactors: Part 2 Shunt reactors[IEC 60289(1988)
IS 5553-3(1990)	Reactors: Part 3 Current limiting reactors and neutral earthing reactors [IEC 60289(1988)
IS 5553-4(1989)	Reactors: Part 4 Damping reactors [IEC 60289(1988)
IS 5553-5(1989)	Reactors: Part 5 Tuning reactors [IEC 60289(1988)
IS 5553-6(1990)	Reactors: Part 6 Earthing transformers (Neutral couplers) [IEC 60289(1988)
IS 5553-7(1990)	Reactors: Part 7 Arc supression reactors [IEC 60289(1988)
IS 5553-8(1990)	Reactors: Part 8 Smoothing reactors [IEC 60289(1988)
IS 5621(1980)	Hollow porcelain isolator or bushing
IS 6160	Rectangular conductors for electrical machine
IS 6162-1(1971)	Paper-Covered Aluminium Conductors - Part I : Round Conductors [IEC 60111]
IS 6162-2(1971)	Paper Covered Aluminium Conductors - Part II : Rectangular Conductors [IEC 60111]
IS 649(1997)	Methods for testing steel sheets for magnetic circuits of power electrical apparatus
IS 7391-2(1974)	Cotton covered copper conductors : Part 2 Rectangular conductors
IS 7421(1974)	Specification for Low Voltage bushings
IS 8468(1977)	On-load tap changers
IS 9335	Specification for Insulating Kraft Paper [IEC 60554]
기타 1.
기타 2.
기타 3.

다. 계전기 및 전력자동화장치

표준번호	제목	검토	번역
IS 11426-1(2006)	Alternating current precision electricity meters for testing purposes : Part 1 Requirements for electro-mechanical meters
IS 11448(2000)	Application Guide for ac Electricity Meters
IS 12346(1999)	Testing Equipment for AC Electrical Energy Meters
IS 13010(2002)	ac Watthour Meters, Class 0.5, 1 and 2 -Specification [IEC 60521:1988]
S 13779(1999)	ac Static Watthour Meters, Class 1 and 2 - Specification [IEC 61036:1996]
IS 14697(1999)	ac Static Transformer Operated Watthour and Var-hour Meters, Class 0.2 S and 0.5 S - Specification
IS 15707(2006)	Testing, evaluation, installation and maintenance of ac electricity meters - Code of practice
IS 15959(2011)	Data Exchange for Electrical Meter - Reading Tariff and Load Control - Companion Specification
IS 1766(1998)	Time Switches for Metering and Load Control [IEC 61038:1992]
IS 8161	Impulse wave testing
IS 9000	Environmental testing
IS 8686(1977)	Static protective relays [IEC 255-4]
기타 1.
기타 2.
기타 3.

라. 케이블 및 피뢰기

표준 번호	표준 제목	검토	번역
IS 10418-1~63	Method of test for cables
IS 12943(1990)	Brass glands for PVC cables
IS 13573(1992)	Joints and Terminations of Polymeric Cables for Working Voltages from 6.6 kV up to and Including 33 kV - Performance Requirements and Type Tests
IS 13705(1993)	Performance requirements and type test for transition joint of cables for working voltages from 11 kV up to and including 33 kV [IEC 60502]
IS 1554-1(1988)	PVC insulated (heavy duty) electric cables: Part 1 For working voltages upto and including 1100 V [IEC 60502:1983]
IS 1554-2(1988)	PVC Insulated (Heavy Duty) Electric Cables - Part 2 : for Working Voltages from 3.3 kV up to and Including 11 kV [IEC 60502:1983]
IS 3961-2(1967)	Recommended current ratings for cables: Part 2 PVC insulated and PVC sheathed heavy duty
IS 3961-3(1968)	Recommended current ratings for cables: Part 3 Rubber insulated cables
IS 3975	Mild steel wires, formed wires and tapes for armouring of cables
IS 398-4(1994)	Aluminium conductors for overhead transmission purposes: Part 4 Aluminium alloy stranded conductors [IEC 60208:1966]
IS 5819(1970)	Recommended short-circuit ratings of high voltage PVC cables
IS 5831(1984)	PVC insulation and sheath of electric cables
IS 6380	Specification of Elastomeric Insulation & Sheath of Electric Cables.
IS 694(2010)	Polyvinyl Chloride Insulated Unsheathed and Sheathed Cables/Cords with RIGID and Flexible Conductor for rated Voltages up to and Including 450/750 V [IEC 60227 - 1 to 5(1979)]
IS 7098-1(1988)	Crosslinked polyethylene insulated PVC sheathed cables: Part 1 For working voltage upto and including 1100 V[IEC 60502:1983]
IS 7098-2(1985) (Amd2-2007)	Crosslink polyethylene insulated PVC sheathed cables: Part 2 For working voltages from 3.3 kV up to and including 33 kV[IEC 60502:1983]
IS 7098-3(1993)	Cross-linked polyethylene insulated thermoplastic sheathed cables: Part 3 For working voltages from 66 kV upto and including 220 kV
IS 8130(1984)	Conductors for Insulated Cables[IEC 60228:1978]
기타 1.
기타 2.
기타 3.

마. 애자 및 금구류

표준 번호	표준 제목	검토	번역
IS 2486-1(1993)	Metal fittings of insulators for overhead power lines with nominal voltage greater than 1000 V: Part 1 General requirements and tests
IS 2486-2(1989)	Insulator fittings for overhead power lines with nominal voltage greater than 1000 V: Part 2 Dimensional requirements [IEC 60120(1984)]
IS 2486-3(1974)	Insulator Fittings for Overhead Power Lines with a Nominal Voltage Greater than 1000 Volts - Part III : Locking Devices [IEC 60372-1(1971)]
IS 2486-4(1981)	Insulator Fittings for Overhead Power Lines with a Nominal Voltage Greater than 1000 V - Part IV : Tests for Locking Devices
IS 3347-4-1(1988)	Dimensions for porcelain transformer bushings for use in lightly polluted atmospheres: Part 4 24 kV bushings, Section 1 Porcelain parts [DIN 42531 to 33]
IS 3347-4-2(1982)	Dimensions for Porcelain Transformer Bushings for Use in Lightly Polluted Atmospheres - Part IV : 24 kV Bushings - Section 2 : Metal Parts
IS 3347-5-1(1979)	Dimensions for Poreclain Transformer Bushings for Use in Lightly Polluted Atmospheres - Part V : 36 kV Bushings - Section 1 : Porcelain Parts
IS 3347-5-2(1979)	Dimensions for Porcelain Transformer Bushings for Use in Normal and Lightly Polluted Atmospheres - Part V : 36 kV Bushings - Section 2 : Metal Parts
IS 3347-8-1(1988)	Dimensions for procelain transformer bushings for use in lightly polluted atmospheres: Part 8 52 kV bushings, Section 1 Porcelain parts
IS 3347-8-2(1988)	Dimensions for procelain transformer bushings for use in lightly polluted atmospheres: Part 8 52 kV bushings, Section 1 Porcelain parts
IS 13134(1992)	Guide for the selection of insulators in respect of polluted conditions. [IEC 60815]
IS 13312(1992)	Dimensions of porcelain oil filled transformer bushings (rated 52 kV) for medium polluted
IS 1363-3(2002)	Hexagon Head Bolts, Screws and Nuts of Product Grade C - Part 3 : Hexagon Nuts
IS 2062(2006)	Hot Rolled low, medium and high tensile structural steel
IS 2071-1(1993)	Methods of High Voltage Testing[IEC : 60060-1 (1989)]
IS 2099(1986)	Bushings for alternating voltages above 1000 Volts
IS 2629(1985)	Recommended practice for Hot Dip Galvanization for iron and steel. [ISO 1461]
IS 2633(1986)	Methods for testing uniformity of coating of zinc coated articles
IS 3203(1982)	Methods of testing of local thickness of electroplated coatings. [ISO 2178]
IS 4699	Specification for refined secondary Zinc
IS 4759(1996)	Hot dip zinc coatings on structural steel & other allied products[ISO 1459, ISO 1461]
IS 5300(1969)	Porcelain Guy Strain Insulators
IS 6745(1972)	Determination of Weight of Zinc Coating on Zinc coated iron and steel articles.[ISO 1460]
IS 731(1971)	Porcelain insulators for overhead power lines with a nominal voltage greater than 1000 V [IEC 60883]
IS 7648(1975)	Silicone compound for application on high voltage porcelain insulators
IS 8263(1976)	Methods of RI Test of HV Insulators[IEC 60437]
기타 1.
기타 2.
기타 3.

바. 기타 번역이 필요하다고 생각되는 표준 및 분야를 적어 주십시오.

① ___________________________________________________________________

② ___________________________________________________________________

③ ___________________________________________________________________

④ ___________________________________________________________________

⑤ ___________________________________________________________________

Ⅲ. 기타 사항

5. 본 연구 및 인도 수출 관련한 제안 사항이 있으면 기술하여 주십시오.

-인도내 제품수요 및 가격경쟁력에 대한 조언 부탁드립니다.

※ 수요조사에 응답해 주셔서 대단히 감사합니다. 설문에 성실히 응답하신 분들에게 본 연구과제의 최종 결과물을 우선적으로 보내드리겠습니다.